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I. Definition of display panel and key
 (
Up
)
 (
Confirm
) (
Menu
)Signal indicator (green)
Error indicator (red)
 (
Down
)

Menu key: enter/return to the main menu
Up key: menu function select up/parameter increment
Down key: menu function select down/parameter decrement
Enter key: select the menu function, and confirm and save when modifying the menu function parameters.
II. Menu function
After the machine is powered on and reset, press the menu key to enter the main menu (exit after 30 seconds of no operation on the main menu interface). See the main menu function table for details (5 main menu options in total); Press the up or down key to select the main menu, press the enter key to modify the function parameters of each menu, and then press the enter key to save the current function parameters (with power-off memory after saving).
	Main menu
	Submenu
	Menu function description

	1. System settings
	1. DMX address
	Modify the DMX address code up or down (the address code can be selected from 001-512), press the Enter key to save, and the default is 001.

	
	2. Encoder
	Up or down to modify the encoder on/off, the confirmation key to save, the default on.

	
	3. X reversal
	Modify X up or down to reverse on/off, enter to save, off by default.

	
	4. Y reversal
	Modify Y up or down to reverse on/off, enter to save, off by default.

	2. Operation mode
	1. Operation mode
	Up or down to select the operating mode DMX/Voice/Auto, enter to save, default to DMX.

	
	2. Channel selection
	Select the channel CH25/CH32/CH53 up or down, press the OK key to save, and the default is CH25.

	3. Manual control

	1. X-axis
	Modify the running parameter value of X motor upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default value is 000.

	
	2. X-axis fine adjustment
	Modify up or down the X fine adjustment motor running parameter value (adjustable range 000-255), press the Enter key to save, and the default is 128.

	
	3. X rotation
	Modify the X rotation parameter value upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	4. Y-axis
	Modify the Y-axis parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	5. Y-axis fine adjustment
	Modify the Y fine adjustment parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	6. XY speed
	Modify the XY speed parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	7. Dimming
	Modify the value of dimming brightness upward or downward (the adjustable range is 000-255). Press the Enter key to save. The default value is 255.

	
	8. Strobe
	Modify the stroboscopic parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	9. Red
	Modify the brightness of the red lamp bead upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	10. Green
	Modify the brightness of the green lamp bead upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	11. Blue
	Modify the brightness of the blue lamp bead upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	12. White
	Modify the brightness of the white lamp bead upward or downward (adjustable range: 000-255), press the confirmation key to save, and the default value is 255.

	
	13. Mode
	Modify the mode parameter value upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default is 000.

	
	14. Speed
	Modify the speed parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	15. Background color
	Modify the parameter value of the background color upward or downward (the adjustable range is 000-255). Press the Enter key to save. The default value is 000.

	
	16. Background tone light
	Modify the background tone light parameter value upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default value is 000.

	
	17. Reset
	When the parameter value is 250-255, the whole machine is reset. The console parameter value must be pulled below 10 and then pushed to 250-255 to be useful. When the parameter value is 000-249, it is useless and cannot be reset.

	4. Display settings
	1. Language selection
	Select Chinese/EN (English) up or down, and press Enter to save. The default is Chinese.

	
	2. Inverted display settings
	Select up or down to close/open the reverse display setting, and press the confirmation key to save. It is closed by default.

	
	3. Screen saver
	Select up or down to turn off/on the screen saver, press the enter key to save, and turn on by default.

	
	4. Software version
	03 VA Program Identifier, not modifiable.

	5. Factory settings
	Display, please enter the password! Change up or down to 138, and then press the confirmation key to enter the factory setting.
	1. X-axis calibration
	Modify the parameter up or down (range: 000-255), press the OK key to save, and the default value is 128.

	
	
	2. Y-axis calibration
	Modify the parameter up or down (range: 000-255), press the OK key to save, and the default value is 128.

	
	
	3. Focus calibration
	Modify the parameter up or down (range: 000-255), press the OK key to save, and the default value is 128.

	
	
	4. Rotation calibration
	Modify the current of the red lamp bead up or down (032-255), press the confirmation key to save, and the default value is 220.

	
	
	5. Red
	Modify the current of the green lamp bead up or down (032-255), press the OK key to save, and the default value is 220.

	
	
	6. Green
	Up or down to modify the blue lamp current (032-255), enter the key to save, default 220.

	
	
	7. Blue
	Up or down to modify the blue lamp current (032-255), enter the key to save, default 220.

	
	
	8. White
	Modify the current of the white lamp bead up or down (032-255), press the OK key to save, and the default value is 220.

	
	
	9. Speed
	Change the speed parameter up or down (range: 000-255), press the OK key to save, and the default value is 065.

	
	
	10. Current
	Select 000/007 up or down, press Enter to save, and the default is 000.

	
	
	11、Logo
	Select 000/001 up or down and press OK to save. The default is 000.

	
	
	12. Temperature
	Change the temperature parameter up or down (range 40-70), press the OK key to save, and the default value is 065.

	
	
	13. Temperature-Fan
	Up or down to select off/on temperature-fan control, enter key to save, default on.



III. Master-slave control
    Two or more identical lamps are connected by DMX three-core signal line, all lamps are modified to any address code from 001 to 512, any one is set as the host, other lamps are slave, and the display screen of all slave does not flicker; When the host computer is used to adjust the effects of gradual change, pulse change, jump change, sound control and self-walking, all slave computers shall synchronize the effects of gradual change, pulse change, jump change, sound control and self-walking.
Special note: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash randomly and not be synchronized.
           2. All lamps must work only when the DMX512 console is turned off.
IV. DMX512 control
After the address codes of all lamps are set, connect all lamps to the DMX512 console in parallel with the DMX three-core signal line. The address code stops flashing, indicating that the DMX512 console signal has been sent to the lamps. Control relevant functions with the DMX512console according to the channel description.
CH25 channel description:
	Passageway
	Channel value
	Basic functions

	1
	000-255
	X-axis

	2
	000-255
	X is not polar

	3
	000-255
	X speed

	4
	000-255
	Y overall

	5
	000-255
	Y mode speed

	6
	000-255
	Y mode

	7
	000-255
	Y-mode amplitude

	8
	000-255
	Y mode direction

	9
	000-255
	Total Dimming (Beam Assist)

	10
	000-255
	Beam stroboscopic

	11
	000-255
	Beam R

	12
	000-255
	Beam G

	13
	000-255
	Beam B

	14
	000-255
	Beam W

	15
	000-255
	Beam pattern

	16
	000-255
	Beam pattern speed

	17
	000-255
	Auxiliary light stroboscopic

	18
	000-255
	Auxiliary light R

	19
	000-255
	Auxiliary light G

	20
	000-255
	Auxiliary light B

	21
	000-255
	Auxiliary light mode

	22
	000-255
	Auxiliary light mode speed

	23
	000-255
	Integrated mode (beam assist)

	24
	000-255
	Integrated pattern speed (beam assist)

	25
	000-255
	Reset: When the parameter value is 250-255, the whole machine is reset. The console parameter value must be pulled below 10 and then pushed to 250-255 to be useful. When the parameter value is 000-249, it is useless and cannot be reset.



CH32 channel description:
	Passageway
	Channel value
	Basic functions

	1
	000-255
	X-axis

	2
	000-255
	X is not polar

	3
	000-255
	X Inching

	4
	000-255
	X speed

	5
	000-255
	Y overall

	6
	000-255
	Y1

	7
	000-255
	Y2

	8
	000-255
	Y3

	9
	000-255
	Y4

	10
	000-255
	Y mode speed

	11
	000-255
	Y mode

	12
	000-255
	Y-mode amplitude

	13
	000-255
	Y mode direction

	14
	000-255
	Total Dimming (Beam Assist) 

	15
	000-255
	Beam stroboscopic

	16
	000-255
	Beam R

	17
	000-255
	Beam G

	18
	000-255
	Beam B

	19
	000-255
	Beam W

	20
	000-255
	Beam pattern

	21
	000-255
	Beam pattern speed

	22
	000-255
	Auxiliary light stroboscopic

	23
	000-255
	Auxiliary light R

	24
	000-255
	Auxiliary light G

	25
	000-255
	Auxiliary light B

	26
	000-255
	Auxiliary light mode

	27
	000-255
	Auxiliary light mode speed

	28
	000-255
	Integrated mode (beam assist)

	29
	000-255
	Integrated pattern speed (beam assist)

	30
	000-255
	Background color (beam assist) 

	31
	000-255
	Background color dimming (beam assist)

	32
	000-255
	Reset: When the parameter value is 250-255, the whole machine is reset. The console parameter value must be pulled below 10 and then pushed to 250-255 to be useful. When the parameter value is 000-249, it is useless and cannot be reset.



CH53 channel description:
	Passageway
	Channel value
	Basic functions

	1
	000-255
	X-axis

	2
	000-255
	X is not polar

	3
	000-255
	X Inching

	4
	000-255
	X speed

	5
	000-255
	Y overall

	6
	000-255
	Y1

	7
	000-255
	Y2

	8
	000-255
	Y3

	9
	000-255
	Y4

	10
	000-255
	Y mode speed

	11
	000-255
	Y mode

	12
	000-255
	Y-mode amplitude

	13
	000-255
	Y mode direction

	14
	000-255
	Total Dimming (Beam Assist) 

	15
	000-255
	Beam stroboscopic

	16
	000-255
	Beam R1

	17
	000-255
	Beam G1

	18
	000-255
	Beam B1

	19
	000-255
	Beam W1

	20
	000-255
	Beam R2

	21
	000-255
	Beam G2

	22
	000-255
	Beam B2

	23
	000-255
	Beam W2

	24
	000-255
	Beam R3

	25
	000-255
	Beam G3

	26
	000-255
	Beam B3

	27
	000-255
	Beam W3

	28
	000-255
	Beam R4

	29
	000-255
	Beam G4

	30
	000-255
	Beam B4

	31
	000-255
	Beam W4

	32
	000-255
	Beam pattern

	33
	000-255
	Beam pattern speed

	34
	000-255
	Auxiliary light stroboscopic

	35
	000-255
	Auxiliary light R1

	36
	000-255
	Auxiliary light G1

	37
	000-255
	Auxiliary light B1

	38
	000-255
	Auxiliary light R2

	39
	000-255
	Auxiliary light G2

	40
	000-255
	Auxiliary light B2

	41
	000-255
	Auxiliary light R3

	42
	000-255
	Auxiliary light G3

	43
	000-255
	Auxiliary light B3

	44
	000-255
	Auxiliary light R4

	45
	000-255
	Auxiliary light G4

	46
	000-255
	Auxiliary light B4

	47
	000-255
	Auxiliary light mode

	48
	000-255
	Auxiliary light mode speed

	49
	000-255
	Integrated mode (beam assist)

	50
	000-255
	Integrated pattern speed (beam assist)

	51
	000-255
	Background color (beam assist) 

	52
	000-255
	? Background color dimming (beam assist) 

	53
	000-255
	Reset: When the parameter value is 250-255, the whole machine is reset. The console parameter value must be pulled below 10 and then pushed to 250-255 to be useful. When the parameter value is 000-249, it is useless and cannot be reset.



V. Technical parameters:
[bookmark: OLE_LINK5]Voltage: AC100 ~ 240V 50/60HZ
Control mode: DMX512, self-propelled, master-slave, voice control, with RDM function.
Channels: CH25, CH32, CH53
Dimming: 32bit 0 ~ 100% linear dimming
Features: XY head + beam + flash + infinite
Working temperature: -30 ℃ ~ 50 ℃
Strobe frequency: 1 ~ 30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP rating: IP20
Dimensions: Height: 26 cm Length: 56 cm Width: 18 cm Weight: 7 kg
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