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I. Definition of display panel and key









Menu key: enter/return to the main menu
Up key: menu function select up/parameter increment
Down key: menu function select down/parameter decrement	
Enter key: select the menu function, and confirm and save when modifying the menu function parameters.
II. Menu function
After the machine is powered on and reset, press the menu key to enter the main menu (exit after 30 seconds of no operation on the main menu interface). See the main menu function table for details (5 main menu options in total); Press the up or down key to select the main menu, press the enter key to modify the function parameters of each menu, and then press the enter key to save the current function parameters (with power-off memory after saving).
	Main menu
	Submenu
	Menu function description

	1. System settings
	1. DMX address
	Modify the DMX address code up or down (the address code can be selected from 001-512), press the Enter key to save, and the default is 001.

	
	2. Encoder
	Up or down to modify the encoder on/off, the confirmation key to save, the default on.

	
	3. X reversal
	Modify X up or down to reverse on/off, enter to save, off by default.

	
	4. Y reversal
	Modify Y up or down to reverse on/off, enter to save, off by default.

	2. Operation mode
	1. Operation mode
	Up or down to select the operating mode DMX/Voice/Auto, enter to save, default to DMX.

	
	2. Channel selection
	Select the channel CH18 up or down, and press CH42 to save. The default is CH18.

	3. Manual control

	1. X-axis
	Modify the running parameter value of X motor upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 128.

	
	2. X rotation
	Modify the X rotation parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	3. X-axis fine adjustment
	Modify up or down the X fine adjustment motor running parameter value (adjustable range 000-255), press the Enter key to save, and the default is 000.

	
	4. Y-axis
	Modify the Y-axis parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	5. Y rotation
	Modify the Y rotation parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	6. Y-axis fine adjustment
	Modify the Y fine adjustment parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	7. XY speed
	Modify the XY speed parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	8. Total dimming
	Modify the total dimming value upward or downward (the adjustable range is 000-255). Press the Enter key to save. The default value is 255.

	
	9. Dimming
	Modify the dimming value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 255.

	
	10. Strobe
	Modify the stroboscopic value upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default value is 000.

	
	11. Red
	Modify the brightness of the red lamp bead upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	12. Green
	Modify the brightness of the green lamp bead upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	13. Blue
	Modify the brightness of the blue lamp bead upward or downward (adjustable range: 000-255). Press the Enter key to save. The default value is 255.

	
	14. White
	Modify the brightness of the white lamp bead upward or downward (adjustable range: 000-255), press the confirmation key to save, and the default value is 255.

	
	15. Mode
	Modify the mode parameter value upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default is 000.

	
	16. Speed
	Modify the speed parameter value upward or downward (adjustable range: 000-255), press the Enter key to save, and the default value is 000.

	
	17. Background color
	Modify the parameter value of the background color upward or downward (the adjustable range is 000-255). Press the Enter key to save. The default value is 000.

	
	18. Background tone light
	Modify the background tone light parameter value upward or downward (the adjustable range is 000-255), press the Enter key to save, and the default value is 000.

	
	19. Reset
	Yes/No

	4. Display settings
	1. Language selection
	Select Chinese/EN (English) up or down, and press Enter to save. The default is Chinese.

	
	2. Inverted display settings
	Select up or down to close/open the reverse display setting, and press the confirmation key to save. It is closed by default.

	
	3. Screen saver
	Select up or down to turn off/on the screen saver, press the enter key to save, and turn on by default.

	
	4. Software version
	The G2FA program identification code cannot be modified.

	5. Factory settings
	Display Please enter the password! Change up or down to 138, and then press the confirmation key to enter the factory setting.
	1. X-axis calibration
	Modify the parameter up or down (range: 000-255), press the OK key to save, and the default value is 128.

	
	
	2. Y-axis calibration
	Modify the parameter up or down (range: 000-255), press the OK key to save, and the default value is 128.

	
	
	3. Red
	Modify the current of the red lamp bead up or down (032-255), press the OK key to save, and the default is 252.

	
	
	4. Green
	Modify the current of the green lamp bead up or down (032-255), press the OK key to save, and the default is 252.

	
	
	5. Blue
	Up or down to modify the blue lamp current (032-255), enter the key to save, the default is 252.

	
	
	6. White
	Modify the current of the white lamp bead up or down (032-255), press the OK key to save, and the default is 252.

	
	
	7. Current
	Select 000/007 up or down, press OK to save, and the default is 004.

	
	
	8. Speed
	Select 000/007 up or down, press Enter to save, and the default is 000.

	
	
	9、Logo
	Select 000/001 up or down and press OK to save. The default is 000.

	
	
	10. Temperature
	Change the temperature parameter up or down (range 40-70), press the OK key to save, and the default value is 065.

	
	
	11. Temperature-Fan
	Up or down to select off/on temperature-fan control, enter key to save, default on.

	
	
	12、LED
	LED light bead sequence selection LEDA/LEDB



III. Master-slave control
    Two or more identical lamps are connected by DMX three-core signal line, all lamps are modified to any address code from 001 to 512, any one is set as the host, other lamps are slave, and the display screen of all slave does not flicker; When the host computer is used to adjust the effects of gradual change, pulse change, jump change, sound control and self-walking, all slave computers shall synchronize the effects of gradual change, pulse change, jump change, sound control and self-walking.
Special note: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash randomly and not be synchronized.
           2. All lamps must work only when the DMX512 console is turned off.
IV. DMX512 control
After the address codes of all lamps are set, connect all lamps to the DMX512 console in parallel with the DMX three-core signal line. The address code stops flashing, indicating that the DMX512 console signal has been sent to the lamps. Control relevant functions with the DMX512console according to the channel description.
CH18 channel description:
	Passageway
	Channel value
	Basic functions

	1
	000-255
	X-axis

	2
	000-255
	The X-axis has no pole

	3
	000-255
	X Fine tuning

	4
	000-255
	Y-axis

	5
	000-255
	The Y-axis has no pole

	6
	000-255
	Y-axis fine adjustment

	7
	000-255
	XY speed

	8
	000-255
	Dimming

	9
	000-255
	Strobe

	10
	000-255
	Red

	11
	000-255
	Green

	12
	000-255
	Blue

	13
	000-255
	White

	14
	000-255
	Pattern

	15
	000-255
	Speed

	16
	000-255
	Background color

	17
	000-255
	Background tonal light

	18
	000-255
	Reset: When the parameter value is 150-255, the whole machine is reset. The console parameter value must be pulled below 10 and then pushed to 150-255 to be useful. When the parameter value is 000-149, it is useless and cannot be reset.


CH42 channel description:
	Passageway
	Channel value
	Basic functions

	1
	000-255
	X-axis

	2
	000-255
	The X-axis has no pole

	3
	000-255
	X Fine tuning

	4
	000-255
	Y-axis

	5
	000-255
	The Y-axis has no pole

	6
	000-255
	Y-axis fine adjustment

	7
	000-255
	XY speed

	8
	000-255
	Dimming

	9
	000-255
	Strobe

	10
	000-255
	Red 1

	11
	000-255
	Green 1

	12
	000-255
	Blue 1

	13
	000-255
	White 1

	14
	000-255
	Red 2

	15
	000-255
	Green 2

	16
	000-255
	Blue 2

	17
	000-255
	White 2

	18
	000-255
	Red 3

	19
	000-255
	Green 3

	20
	000-255
	Blue 3

	21
	000-255
	White 3

	22
	000-255
	Red 4

	23
	000-255
	Green 4

	24
	000-255
	Blue 4

	25
	000-255
	White 4

	26
	000-255
	Red 5

	27
	000-255
	Green 5

	28
	000-255
	Blue 5

	29
	000-255
	White 5

	30
	000-255
	Red 6

	31
	000-255
	Green 6

	32
	000-255
	Blue 6

	33
	000-255
	White 6

	34
	000-255
	Red 7

	35
	000-255
	Green 7

	36
	000-255
	Blue 7

	37
	000-255
	White 7

	38
	000-255
	Pattern

	39
	000-255
	Speed

	40
	000-255
	Background color

	41
	000-255
	Background tonal light

	42
	000-255
	Reset: When the parameter value is 150-255, the whole machine is reset. The console parameter value must be pulled below 10 and then pushed to 150-255 to be useful. When the parameter value is 000-149, it is useless and cannot be reset.




V. Technical parameters:
[bookmark: OLE_LINK5]Voltage: AC100 ~ 240V 50/60HZ
Power: 180W
Lamp beads: 7 4-in-1 lamp beads
Control mode: DMX512, self-propelled, master-slave, voice control, with RDM function.
Channel: CH18, CH42
Dimming: 32bit 0 ~ 100% linear dimming
Features: XY head + beam + flash + XY stepless
Working temperature: -30 ℃ ~ 50 ℃
Strobe frequency: 1 ~ 30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP rating: IP20
Dimensions: Height: 23.5cm Length: 58 cm Width: 18 cm Weight: 5.9 kg
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